1. Minimum duty cycle value: 1.0. Maximum duty cycle value: 11.0.
2. Try statement: All the statements are executed until an exception occurs.

Except statement: Handles the KeyboardInterrupt exception.

Finally statement: Allows the running and execution of commands that come after, that can run despite exception occurrences.